Release Notes - FT638 Digital Radio Box						FunkTronic - 2024

(SEP = only valid for Sepura TETRA radios, MOT = only valid for Motorola TETRA radios)

V1.01 05.06.2018
	- integration of group selection via 4-digit SEP number
	- LAN access to PEI AT interface (needs option EXTENDED)
	  (STD version: 1x access to MRT1/MRT2, I/O version: 2x access to MRT1)
	- third-party access to x VOIP connections per ETH socket (ACCESS:1x, EXTENDED:4x, FULL: all)
	- NonBOS-Version (SW name = "FT638 NB")

V1.01 27.09.2018
	- improvements for call processing routines
	- minor update of IP stack
	- minor bugfixes for web interface
	- FIX: readout procedure adapted for MRTs with deactivated DMO capability

V1.01 15.11.2018
	- FIX: data for "recent groups" folder is now retained after cold reset
	- version with English web interface now available
	- FIX: potential restart loop directly after firmware update

V1.01 16.01.2019
	- streamlining of PEI multiplexer: same output behavior for all PEI AT interfaces
	- FIX-MOT: SIM data handling for MRTs with configured internal and external SIM capability


V1.02 21.03.2019
	- PID 204 implemented as an alternative source (to PID 220) of status acknowledgement texts (Home Mode)
	- SEP: automatic status target request implemented (V10.020 and newer)
	- FIX-MOT: automatic status target request handling fixed for new codeplug versions
	- PEI multiplexer also replicates OK and ERROR, if AT echo is active
	- minor improvements on internal data handling and protocol compatibility to FT636B

V1.02 18.04.2019
	- FIX: transmission of status reenabled (not possible in V1.02/21.03.19)

V1.03 23.07.2019
	- general performance update for IP stack, especially important for larger assemblies 
	- FIX-SEP (V10.020): PEI-AT connection was ceased permanently (restart of SRG3900 necessary), when trying to send in DMO during incoming call
	- FIX-MOT: in rare cases MRT was powering off during operation


V1.04 28.05.2020
	- FIX: audio routing directly after startup and in sophisticated setups fixed
	- full implementation of SDS memory and display
	- SEP: SDS can now be received by FT638 and Sepura Consoles simultaneously
	- SEP: Group calls now possible in Repeater Mode

V1.04 03.09.2020
	- SEP: readout for TMOa groups (groups with different MNI)
	- SEP: automatic network switching for easy activation of TMOa groups implemented
	- minor bugfixes

V1.05 03.03.2021
	- MOT: automatic TMO-network change now also possible without connection

V1.06 25.11.2021
	- first unified TETRA+DMR codebase version (but still as separate TETRA or DMR versions)
	- first DMR support for MOTOTRBO and Kenwood DMR/Nexedge

V1.06 07.02.2022
	- Hytera DMR support added

V1.06 27.07.2022
	- several improvements and minor bugfixes, mainly for DMR functionality
	- improvements in SDS-TL handling: timestamp and internal 0xFF(ÿ) characters
	- FIX-MOT: sporadic errors in status target requests could lead to system reboot

V1.07 26.07.2023
	- connectivity for ICOM DPMR radios added
	- unified firmware with enhanced MRT configuration for TETRA or DMR radios
	- ethernet/internet time server connectivity for time display in DMR setups
	- configuration of SQL logics on A1/A2 connectors
	- group functionality for VoIP connections (optimized audio settings in multi-room arrangements)
	- fix for problems with new browser versions
	- talking in repeater mode enabled for all TETRA radios (if possible with MRT codeplug/firmware)
	- MOT: display of phonebook entries instead of OPTAs if available
	- in folder "recent groups"/"Letzte Gruppen": automatic switching between DMO/TMO groups implemented

V1.08 22.03.2024
	- fix for default values of new page "MRT configuration"
	- improved handling of PTT requests (TETRA)
	- PEI communication is now visible via syslog level "medium" or higher

V1.08 20.06.2024
	- Minor bugfixes
	- general improvements for TETRA comms logic and PEI multiplexer
	- BUGFIX: occasional cases of deteriorated incoming AF signal solved
 	  (only observed directly after power-on when operating via MRT2 on an IN/OUT-Version)

V1.08 04.10.2024
	- Connectors A1/A2: audio lines to and from the radio are now always connected
	  (before, PTT confirmation tones of TETRA/DMR could not be heard on A1/A2)

V1.08 21.11.2024
	- Bugfix: Web-Interface for subsections "SDS" and "PEI->VoIP" on appl. page 2
	- Bugfix: SDS Cleanup Procedure could result in cut-off for longer messages
	- Bugfix-CRITICAL: Emergency Call PTT Handling in TMO mode fixed (affected: all previous V1.08 versions)